We want to compare the computers R1 and R2, which differ that R1 has the machine instructions for the floatingpoint operations, while R2 has not (FP operations are implemented in the software using several non-FP instructions). Both computers have a clock frequency of 400 MHz. In both we perform the same program, which has the following mixture of commands